;
;
; Installs WinUsb
;

[Version]
Signature = "$Windows NT$"
Class     = KmWinUSB
ClassGUID = {F3ACB5C9-5685-4f07-96B5-89C5B22CB436}
Provider  = %ManufacturerName%
CatalogFile = KmWinUSB1.cat
DriverVer=09/04/2012,13.54.20.543

; ========== Manufacturer/Models sections ===========

[Manufacturer]
%ManufacturerName% = KDCWINUSB,NTx86.6.0,NTamd64.6.0

[KDCWINUSB.NTx86.6.0]
"Kyocera ECOSYS MA4000x"       = USB_Install,USB\VID_0482&PID_0de0&MI_02
"Kyocera ECOSYS MA4000fx"      = USB_Install,USB\VID_0482&PID_0de1&MI_02
"Kyocera ECOSYS MA4000wfx"     = USB_Install,USB\VID_0482&PID_0de2&MI_02
"Kyocera ECOSYS MA4000wifx"    = USB_Install,USB\VID_0482&PID_0de3&MI_02
"Kyocera ECOSYS PA4000x"       = USB_Install,USB\VID_0482&PID_0de9&MI_01
"Kyocera ECOSYS PA4000wx"      = USB_Install,USB\VID_0482&PID_0dea&MI_01
"Kyocera ECOSYS MA4000wfx(J)"  = USB_Install,USB\VID_0482&PID_0de4&MI_02
"Kyocera ECOSYS MA4000wifx(J)" = USB_Install,USB\VID_0482&PID_0de5&MI_02
"Kyocera ECOSYS PA4000wx(J)"   = USB_Install,USB\VID_0482&PID_0deb&MI_01
"Kyocera ECOSYS MA3501wfx"   = USB_Install,USB\VID_0482&PID_0e34&MI_02
"Kyocera ECOSYS MA3500wfx"   = USB_Install,USB\VID_0482&PID_0e36&MI_02
"Kyocera ECOSYS MA3500fx"    = USB_Install,USB\VID_0482&PID_0e37&MI_02
"Kyocera ECOSYS MA3500x"     = USB_Install,USB\VID_0482&PID_0e38&MI_02
"Kyocera ECOSYS PA3500wx"    = USB_Install,USB\VID_0482&PID_0e3a&MI_01
"Kyocera ECOSYS PA3500x"     = USB_Install,USB\VID_0482&PID_0e3c&MI_01

[KDCWINUSB.NTamd64.6.0]
"Kyocera ECOSYS MA4000x"       = USB_Install,USB\VID_0482&PID_0de0&MI_02
"Kyocera ECOSYS MA4000fx"      = USB_Install,USB\VID_0482&PID_0de1&MI_02
"Kyocera ECOSYS MA4000wfx"     = USB_Install,USB\VID_0482&PID_0de2&MI_02
"Kyocera ECOSYS MA4000wifx"    = USB_Install,USB\VID_0482&PID_0de3&MI_02
"Kyocera ECOSYS PA4000x"       = USB_Install,USB\VID_0482&PID_0de9&MI_01
"Kyocera ECOSYS PA4000wx"      = USB_Install,USB\VID_0482&PID_0dea&MI_01
"Kyocera ECOSYS MA4000wfx(J)"  = USB_Install,USB\VID_0482&PID_0de4&MI_02
"Kyocera ECOSYS MA4000wifx(J)" = USB_Install,USB\VID_0482&PID_0de5&MI_02
"Kyocera ECOSYS PA4000wx(J)"   = USB_Install,USB\VID_0482&PID_0deb&MI_01
"Kyocera ECOSYS MA3501wfx"   = USB_Install,USB\VID_0482&PID_0e34&MI_02
"Kyocera ECOSYS MA3500wfx"   = USB_Install,USB\VID_0482&PID_0e36&MI_02
"Kyocera ECOSYS MA3500fx"    = USB_Install,USB\VID_0482&PID_0e37&MI_02
"Kyocera ECOSYS MA3500x"     = USB_Install,USB\VID_0482&PID_0e38&MI_02
"Kyocera ECOSYS PA3500wx"    = USB_Install,USB\VID_0482&PID_0e3a&MI_01
"Kyocera ECOSYS PA3500x"     = USB_Install,USB\VID_0482&PID_0e3c&MI_01

; ========== Class definition ===========

[ClassInstall32]
AddReg = ClassInstall_AddReg

[ClassInstall_AddReg]
HKR,,,,%ClassName%
HKR,,NoInstallClass,,1
HKR,,IconPath,%REG_MULTI_SZ%,"%%systemroot%%\system32\setupapi.dll,-20"
HKR,,LowerLogoVersion,,5.2

; =================== Installation ===================

[USB_Install]
Include = winusb.inf
Needs   = WINUSB.NT

[USB_Install.Services]
Include =winusb.inf
Needs   = WINUSB.NT.Services

[USB_Install.HW]
AddReg=Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{9f543223-cede-4fa3-b376-a25ce9a30e74}"


; [DestinationDirs]
; If your INF needs to copy files, you must not use the DefaultDestDir directive here.  
; You must explicitly reference all file-list-section names in this section.

; =================== Strings ===================

[Strings]
ManufacturerName="KYOCERA Document Solutions Inc."
ClassName="Universal Serial Bus devices"
DeviceName="Kyocera WINUSB"
REG_MULTI_SZ = 0x00010000

