;================================================================
;
;  OEMSETUP.INF (PCLDriver)
;
;  Kyocera PCL Mini-Driver Installation Script
;  Windows 10, 11
;  Windows Server 2016, 2019, 2022
;  Languages: English, French, German, Italian, Korean,
;             Portuguese, and Spanish
;  Plug & Play Version
;
;  (C) 2025 KYOCERA Document Solutions Inc.
;
;================================================================

;----------------------------------------------------------------
; Version Section
;----------------------------------------------------------------
;
[Version]
Signature  = "$Windows NT$"
Class      = Printer
ClassGUID  = {4D36E979-E325-11CE-BFC1-08002BE10318}
Provider   = "KYOCERA Document Solutions Inc."
CatalogFile=KYOCERA.CAT
DriverVer  = 10/07/2024,1.6
DriverIsolation=2

;
; Manufacturer section.
;
; This section lists all of the manufacturers
; that we will display in the Dialog box
;
[Manufacturer]
"Kyocera"=Kyocera,NTx86.6.0,NTamd64.6.0,NTia64.6.0

;
; Model sections.
;
; Each section here corresponds with an entry listed in the
; [Manufacturer] section, above. The models will be displayed in the order
; that they appear in the INF file.
;

[Kyocera.NTx86.6.0]
"Kyocera ECOSYS MA4000wifx"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_MA4000B156
"Kyocera ECOSYS MA4000wifx"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_MA4000B156

"Kyocera ECOSYS MA4000wfx"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_MA4000AF41
"Kyocera ECOSYS MA4000wfx"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_MA4000AF41

"Kyocera ECOSYS MA4000fx"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_MA40001A60
"Kyocera ECOSYS MA4000fx"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_MA40001A60

"Kyocera ECOSYS MA4000x"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_MA400028DF
"Kyocera ECOSYS MA4000x"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_MA400028DF

"Kyocera ECOSYS PA4000x"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_PA40002912
"Kyocera ECOSYS PA4000x"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_PA40002912

"Kyocera ECOSYS PA4000wx"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_PA4000DFAC
"Kyocera ECOSYS PA4000wx"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_PA4000DFAC

"Kyocera ECOSYS MA3501wfx"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_MA3501C634
"Kyocera ECOSYS MA3501wfx"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_MA3501C634

"Kyocera ECOSYS MA3500wfx"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_MA35003A35
"Kyocera ECOSYS MA3500wfx"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_MA35003A35

"Kyocera ECOSYS MA3500fx"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_MA3500ADAD
"Kyocera ECOSYS MA3500fx"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_MA3500ADAD

"Kyocera ECOSYS MA3500x"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_MA3500246A
"Kyocera ECOSYS MA3500x"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_MA3500246A

"Kyocera ECOSYS PA3500x"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_PA350047A6
"Kyocera ECOSYS PA3500x"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_PA350047A6

"Kyocera ECOSYS PA3500wx"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_PA3500A8C2
"Kyocera ECOSYS PA3500wx"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_PA3500A8C2

[Kyocera.NTamd64.6.0]
"Kyocera ECOSYS MA4000wifx"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_MA4000B156
"Kyocera ECOSYS MA4000wifx"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_MA4000B156

"Kyocera ECOSYS MA4000wfx"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_MA4000AF41
"Kyocera ECOSYS MA4000wfx"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_MA4000AF41

"Kyocera ECOSYS MA4000fx"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_MA40001A60
"Kyocera ECOSYS MA4000fx"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_MA40001A60

"Kyocera ECOSYS MA4000x"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_MA400028DF
"Kyocera ECOSYS MA4000x"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_MA400028DF

"Kyocera ECOSYS PA4000x"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_PA40002912
"Kyocera ECOSYS PA4000x"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_PA40002912

"Kyocera ECOSYS PA4000wx"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_PA4000DFAC
"Kyocera ECOSYS PA4000wx"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_PA4000DFAC

"Kyocera ECOSYS MA3501wfx"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_MA3501C634
"Kyocera ECOSYS MA3501wfx"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_MA3501C634

"Kyocera ECOSYS MA3500wfx"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_MA35003A35
"Kyocera ECOSYS MA3500wfx"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_MA35003A35

"Kyocera ECOSYS MA3500fx"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_MA3500ADAD
"Kyocera ECOSYS MA3500fx"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_MA3500ADAD

"Kyocera ECOSYS MA3500x"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_MA3500246A
"Kyocera ECOSYS MA3500x"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_MA3500246A

"Kyocera ECOSYS PA3500x"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_PA350047A6
"Kyocera ECOSYS PA3500x"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_PA350047A6

"Kyocera ECOSYS PA3500wx"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_PA3500A8C2
"Kyocera ECOSYS PA3500wx"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_PA3500A8C2

[Kyocera.NTia64.6.0]
"Kyocera ECOSYS MA4000wifx"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_MA4000B156
"Kyocera ECOSYS MA4000wifx"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_MA4000B156

"Kyocera ECOSYS MA4000wfx"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_MA4000AF41
"Kyocera ECOSYS MA4000wfx"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_MA4000AF41

"Kyocera ECOSYS MA4000fx"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_MA40001A60
"Kyocera ECOSYS MA4000fx"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_MA40001A60

"Kyocera ECOSYS MA4000x"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_MA400028DF
"Kyocera ECOSYS MA4000x"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_MA400028DF

"Kyocera ECOSYS PA4000x"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_PA40002912
"Kyocera ECOSYS PA4000x"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_PA40002912

"Kyocera ECOSYS PA4000wx"		= ECMA4000.6.0,USBPRINT\KyoceraECOSYS_PA4000DFAC
"Kyocera ECOSYS PA4000wx"		= ECMA4000.6.0,WSDPRINT\KyoceraECOSYS_PA4000DFAC

"Kyocera ECOSYS MA3501wfx"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_MA3501C634
"Kyocera ECOSYS MA3501wfx"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_MA3501C634

"Kyocera ECOSYS MA3500wfx"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_MA35003A35
"Kyocera ECOSYS MA3500wfx"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_MA35003A35

"Kyocera ECOSYS MA3500fx"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_MA3500ADAD
"Kyocera ECOSYS MA3500fx"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_MA3500ADAD

"Kyocera ECOSYS MA3500x"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_MA3500246A
"Kyocera ECOSYS MA3500x"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_MA3500246A

"Kyocera ECOSYS PA3500x"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_PA350047A6
"Kyocera ECOSYS PA3500x"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_PA350047A6

"Kyocera ECOSYS PA3500wx"		= ECMA3500.6.0,USBPRINT\KyoceraECOSYS_PA3500A8C2
"Kyocera ECOSYS PA3500wx"		= ECMA3500.6.0,WSDPRINT\KyoceraECOSYS_PA3500A8C2
;
; Installer Sections
;
; These sections control file installation, and reference all files that
; need to be copied. The section name will be assumed to be the driver
; file, unless there is an explicit DriverFile section listed.
;

[ECMA4000.6.0]
CopyFiles=@ECMA4000.GPD,Resources
CopyFiles=AutoConfig,@ECMA4000.GDL
DataFile=ECMA4000.GPD
CoreDriverSections="{D20EA372-DD35-4950-9ED8-A6335AFE79F0},UNIDRV_BIDI.OEM,UNIDRV_BIDI_DATA,TTFSUB.OEM"

[ECMA3500.6.0]
CopyFiles=@ECMA3500.GPD,Resources
CopyFiles=AutoConfig,@ECMA4000.GDL
DataFile=ECMA3500.GPD
CoreDriverSections="{D20EA372-DD35-4950-9ED8-A6335AFE79F0},UNIDRV_BIDI.OEM,UNIDRV_BIDI_DATA,TTFSUB.OEM"


; Copy Sections
;
; Lists of files that are actually copied. These sections are referenced
; from the installer sections, above. Only create a section if it contains
; two or more files (if we only copy a single file, identify it in the
; installer section, using the @filename notation) or if it's a color
; profile (since the DestinationDirs can only handle sections, and not
; individual files).

[Resources]
kyfont4.dll
kyres14.dll

[AutoConfig]
kyauto09.ini
kyqury09.xml

[PrinterPackageInstallation.x86]
PackageAware=TRUE
CoreDriverDependencies={D20EA372-DD35-4950-9ED8-A6335AFE79F0}

[PrinterPackageInstallation.amd64]
PackageAware=TRUE
CoreDriverDependencies={D20EA372-DD35-4950-9ED8-A6335AFE79F0}

[PrinterPackageInstallation.ia64]
PackageAware=TRUE
CoreDriverDependencies={D20EA372-DD35-4950-9ED8-A6335AFE79F0}

;
; Call SetupSetDirectoryId with 66000 to set the target directory at runtime
; (depending on which environment drivers are getting installed)
;

[DestinationDirs]
DefaultDestDir=66000

[SourceDisksNames.x86]
1 = %Disk1%,,,""

[SourceDisksNames.amd64]
1 = %Disk1%,,,""

[SourceDisksNames.ia64]
1 = %Disk1%,,,""

[SourceDisksFiles]
ECMA4000.gdl	= 1
ECMA4000.gpd	= 1
ECMA3500.gpd	= 1
kyfont4.dll		= 1
kyres14.dll		= 1
kyauto09.ini 	= 1
kyqury09.xml	= 1

;
; Localizable Strings
;

[Strings]
Disk1 = "Kyocera CD-ROM"
